



1. 800ppbv BTEX 0.2min










1. BTEX 800ppbv 0.5min






1. BTEX 800ppbv 1min










1. BTEX 800ppbv 2min


Update software again to improve temperature profile








1. BTEX 800ppbv 5min (toluene, ethylbenzene, xylenes are all saturated; benzene is not increased proportionally.





1. Air after filter

