


1. Air after filter






1. Canister test


This is 200ppbv after 4 times cleaning




After another 4 times





1. 1000ppbv 0.2min




1. 1000ppbv 0.5min#1










3. 1000ppbv BTEX 1min










4. 1000ppbv BTEX 2min








1. 1000ppbv BTEX 5min





1. Air after filter

